NMS-SD3-AM180X

Technical Specifications

Main technical specifications

Form factor	SODIMM 204 EDGE
CPU	Texas Instruments Sitara ARM microprocessors: AM1808/AM1806/AM1802/AM1810
ARM frequencies: 300MHz - 356MHz
Texas Instruments C6000 DSP+ARM Processor: OMAP-L138/OMAP-L132
DSP+ARM frequencies: 200MHz - 456MHz
RAM	DDR2-150MHz 64MB / 128MB / 256MB
FLASH	NAND FLASH 128MB / 256MB / 512MB / 1GB
EEPROM	I2C serial EEPROM 256byte, Unique ID
Power Management IC	TPS65070
Interfaces	USB Full-speed host, USB OTG
EMAC - RMII/MII interface
SATA - 1.5Gbps, 3.0Gbps
MMC/SD - 2 controllers
UART(SCI) - 3 channel
PWM - 2 channel
eCAP - 3 channel
I2C - 2 controllers
HPI - one 16-bit interface
uPP (universal parallel port)
McBSP - 2 channel
McASP - 1 channel
SPI - 2 controllers
Power supply voltage	TBD
Power consumption	TBD
Dimensions	TBD

Block Diagram

Module block diagram

Processor

Module block diagram

PMIC notes

Charger/Power Path Management - Linear charger, Thermal regulation, Safety timers, Temperature Sense Input

wLED boost converter - Up to 2 x 10 Leds, up to 25ma per String

Touch Screen interface - I2C bus, 10-bit ADX

Undervoltage Lockout and Battery fault comparator