Power

MOSFET driver, MOSFET transistors

Vout	VREF	Rtop	Rbot	err, %	Vout
1.5V	0.6V	49K9	33K	0.47	1.51V
5V	10K	1K37	-0.41	4.98V
0.9V	0.8V
1V	1K5	6K04	-0.13	0.999V
1.2V	1K5	3K	0	1.2V
1.8V	4K99	3K92	1.02	1.82V
2.5V	24K9	11K8	-0.47	2.49V
4K7	2K2	0.36	2.51V
3.3V	4K7	1K5	0.2	3.31V
24K9	7K87	0.94	3.33V
5V	15K	2K8	1.71	5.09V

Manufacturers

Anpec	china\taiwan
Mikron	russia

LDO

DCDC boost

link	ext	description	manufacturer	version	date	lang
FAIR-S-A0000507963-1.pdf	pdf	FAN48623 Onsemi (Fairchild) 2500 mA Boost DCDC with Bypass Mode	Onsemi (Fairchild)	rev. 1.7	2015.03	EN

DCDC buck

FAN53200-D.PDF	PDF	FAN53200 Onsemi TinyBuck Regulator, Digitally Programmable, 5 A, 2.4 MHz	Onsemi	rev. 3	2020.05	EN
NCP1597B-D.PDF	PDF	NCP1597B Onsemi Buck Regulator - Synchronous 1 MHz, 2 A	Onsemi	rev. 2	2019.08	EN
PAM2305.pdf	pdf	PAM2305 Diodes 1A STEP-DOWN DC-DC CONVERTER	Diodes	rev. 2-6	2013.01	EN
TCS4525_Ver.1.0.pdf	pdf	TCS4525 DCDC 5A 3MHz I2C (FAN53200UC35X analog)	TCS	v1	2015.05.26	EN

DCDC Controller

NCP1589A	TPS51113	ISL6341, ISL6341C	300kHz
NCP1589A	TPS51163	ISL6341A, ISL6341B	600kHz

DC/DC (AC/DC) Convertor

KP321XB.PDF	PDF	KP321XB KIWI KP321XB series is a high-performance and low-cost PWM control function	KIWI	-	-	CN
MP9488.PDF	PDF	MP9488 MPS The MP9488 is a 7.5V to 450V, wide input, 300mA, step-down converter	MPS	rev. 1	2016.12	EN
BM2P129TF.PDF	PDF	BM2P129TF ROHM The PWM type DC/DC converter for AC/DC This series has a built-in HV starter circuit that tolerates 650V/800V	ROHM	rev. 2	2017.04	EN
RAA223012.PDF	PDF	RAA223012 Renesas The RAA223012 is a universal input AC/DC switching buck regulator with ultra-low standby power that features a 700V integrated MOSFET capable of delivering up to 2.5W output power. It supports output voltage as low as 3.3V.	Renesas	rev. 3.01	2022.03	EN
AL17050.PDF	PDF	AL17050 Diodes The AL17050 is a universal AC high voltage input step down regulator Working with a single winding inductor and integrating a 500V	Diodes	rev. 2 - 2	2018.04	EN
BM2P1xxTF.PDF	PDF	BM2P1xxTF ROHM The PWM type DC/DC converter for AC/DC This series has a built-in HV starter circuit that tolerates 650V/800V	ROHM	rev. 2	2017.04	EN
LSxx-K3BxxSS.PDF	PDF	LSxx-K3BxxSS MORNSUN LSxx-K3BxxSS series is highly efficient green power AC-DC Converter series. It features wide input voltage range, accepting both DC and AC input voltage, high efficiency and low power consumption.	MORNSUN	A/3	2023.03	EN