Rockchip RV1103 RV1106

Overview

boot	https://opensource.rock-chips.com/wiki_Boot_option
rkbin	https://github.com/rockchip-linux/rkbin/blob/master/RKBOOT/RV1106MINIALL_EMMC_TB.ini
rkdeveloptool	https://opensource.rock-chips.com/wiki_Rkdeveloptool
rockusb	https://opensource.rock-chips.com/wiki_Rockusb
boot\emmc\u-boot\…	https://blog.csdn.net/qq_28877125/article/details/132999147
sdcard + sdio	https://blog.csdn.net/qq_28877125/article/details/133634104
sdcard boot	https://wiki.luckfox.com/Luckfox-Pico/Luckfox-Pico-Plus-SD
luckfox download	https://wiki.luckfox.com/Luckfox-Pico/Datasheets/
luckfox info	https://www.spotpear.com/index/study/detail/id/1100.html

Boot

Boot from SPI flash means firmware for stage 2 and 3(SPL and U-Boot only) in SPI flash and stage 4/5 in other place;

Struct

Docs

link	ext	description	version	date	lang

Pinout RV1103G1

Pin Name	Pin	Bank	Group
MIPI_CLK0_OUT/GPIO3_C4_d	1	GPIO3
GPIO3_C5_d	2	GPIO3
PWM7_IR_M2/MIPI_CLK1_OUT/GPIO3_C6_d	3	GPIO3
I2C4_SCL_M2/UART5_TX_M2/GPIO3_C7_d	4	GPIO3
I2C4_SDA_M2/UART5_RX_M2/GPIO3_D0_d	5	GPIO3
DVDD_1	6	CORE	PWR
GPIO4_VCC3V3	7	GPIO4	PWR
SDMMC0_DET/GPIO3_A1_u	8	GPIO3
SDMMC0_D1/UART2_TX_M0/PWM9_M0/GPIO3_A2_u	9	GPIO3
SDMMC0_D0/UART2_RX_M0/PWM8_M0/GPIO3_A3_u	10	GPIO3
SDMMC0_CLK/UART5_RTSN_M0/I2C0_SCL_M2/PWM10_M0/GPIO3_A4_d	11	GPIO3
SDMMC0_CMD/UART5_CTS_M0/I2C0_SDA_M2/PWM11_IR_M0/GPIO3_A5_u	12	GPIO3
SDMMC0_D3/UART5_TX_M0/JTAG_CPU_TMS_M0/JTAG_HPMCU_TMS_M1/GPIO3_A6_u	13	GPIO3
SDMMC0_D2/UART5_RX_M0/JTAG_CPU_TCK_M0/JTAG_HPMCU_TCK_M1/GPIO3_A7_u	14	GPIO3
SARADC_IN1/PWM1_M1/GPI4_C1_z	15	GPI4
SARADC_IN0/GPI4_C0_z	16	GPI4
SARADC_USB_AVDD1V8	17	USB	PWR
USB_DM	18	USB	USB
USB_DP	19	USB	USB
USB_AVDD3V3	20	USB	PWR
CODEC_LINEOUT	21	CODEC	AUDIO
CODEC_VCM	22	CODEC	AUDIO
CODEC_AVDD1V8	23	CODEC	AUDIO
CODEC_MIC0P_MICP	24	CODEC	AUDIO
CODEC_MICBIAS	25	CODEC	AUDIO
CODEC_MIC1P_MICN	26	CODEC	AUDIO
GPIO3_VCC	27	GPIO3	PWR
FSPI_D3/GPIO4_A6_u	28	GPIO4
FSPI_D0/GPIO4_A4_u	29	GPIO4
FSPI_D1/GPIO4_A3_u	30	GPIO4
FSPI_D2/GPIO4_A2_u	31	GPIO4
FSPI_CS0/GPIO4_B0_u	32	GPIO4
FSPI_CLK/GPIO4_B1_d	33	GPIO4
DDR_VDDQ_1	34	DDR	PWR
DDR_VDDQ_2	35	DDR	PWR
DVDD_2	36	CORE	PWR
DRAM_ZQ	37	DDR	SYS
DDR_PLL_AVDD1V8	38	DDR	PWR
DVDD_3	39	CORE	PWR
DDR_VDDQ_3	40	DDR	PWR
TVSS	41	PWR
PWR_CTRL_M0/PWM1_M0/GPIO0_A4_d	42	GPIO0
PMU_VCC3V3	43	PWR
OSC_PLL_PMU_DVDD	44	CLK	PWR
OSC_XIN	45	CLK	CLK
OSC_XOUT	46	CLK	CLK
OSC_AVDD1V8/PLL_AVDD1V8	47	CLK	PWR
PWM0_M0/CPU_AVS/GPIO1_A2_d	48	GPIO1
JTAG_CPU_TCK_M1/UART2_TX_M1/JTAG_HPMCU_TCK_M0/GPIO1_B2_d	49	GPIO1
JTAG_CPU_TMS_M1/UART2_RX_M1/JTAG_HPMCU_TMS_M0/GPIO1_B3_u	50	GPIO1
GPIO1_VCC3V3	51	GPIO1	PWR
PWM10_M1/UART4_RTSN_M1/GPIO1_C6_d	52	GPIO1
PWM11_IR_M1/UART4_CTSN_M1/GPIO1_C7_d	53	GPIO1
I2C3_SCL_M1/UART5_TX_M1/PWM11_IR_M2/AUD_DSM_N/GPIO1_D3_d	54	GPIO1
I2C3_SDA_M1/UART5_RX_M1/SPI0_CS1_M0/PWM0_M1/AUD_DSM_P/GPIO1_D2_d	55	GPIO1
PWM10_M2/UART5_CTS_M1/UART3_RX_M1/GPIO1_D1_d	56	GPIO1
PWM3_IR_M2/UART5_RTS_M1/UART3_TX_M1/GPIO1_D0_d	57	GPIO1
DVDD_4	58	CORE	PWR
GPIO6_VCC	59	GPIO6	PWR
PWM9_M1/UART4_TX_M1/SDMMC1_D2_M1/GPIO1_C5_d	60	GPIO1
PWM8_M1/UART4_RX_M1/SDMMC1_D3_M1/GPIO1_C4_d	61	GPIO1
PWM6_M2/I2C4_SDA_M1/SDMMC1_CMD_M1/SPI0_MISO_M0/GPIO1_C3_d	62	GPIO1
PWM5_M2/I2C4_SCL_M1/SDMMC1_CLK_M1/SPI0_MOSI_M0/GPIO1_C2_d	63	GPIO1
PWM4_M2/SPI0_CLK_M0/SDMMC1_D0_M1/GPIO1_C1_d	64	GPIO1
PWM2_M2/SPI0_CS0_M0/SDMMC1_D1_M1/GPIO1_C0_d	65	GPIO1
OTP_AVDD1V8/ETH_AVDD1V8/TSADC_AVDD1V8	66	PWR
ETH_PHY_RXN	67	ETH	ETH
ETH_PHY_RXP	68	ETH	ETH
ETH_PHY_TXN	69	ETH	ETH
ETH_PHY_TXP	70	ETH	ETH
ETH_AVDD3V3	71	ETH	PWR
ETH_EXTR	72	ETH	ETH
DVDD_5	73	CORE	PWR
CPU_DVDD	74	CORE	PWR
DVDD_6	75	CORE	PWR
MIPI_CSI_RX_D3N/LVDS_RX_D3N/GPI3_B0_d	76	GPI3
MIPI_CSI_RX_D3P/LVDS_RX_D3P/GPI3_B1_d	77	GPI3
MIPI_CSI_RX_CK1N/LVDS_RX_CK1N/GPI3_B2_d	78	GPI3
MIPI_CSI_RX_CK1P/LVDS_RX_CK1P/GPI3_B3_d	79	GPI3
MIPI_CSI_RX_D2N/LVDS_RX_D2N/GPI3_B4_d	80	GPI3
MIPI_CSI_RX_D2P/LVDS_RX_D2P/GPI3_B5_d	81	GPI3
MIPI_CSI_RX_D1N/LVDS_RX_D1N/GPI3_B6_d	82	GPI3
MIPI_CSI_RX_D1P/LVDS_RX_D1P/GPI3_B7_d	83	GPI3
MIPI_CSI_RX_CK0N/LVDS_RX_CK0N/GPI3_C0_d	84	GPI3
MIPI_CSI_RX_CK0P/LVDS_RX_CK0P/GPI3_C1_d	85	GPI3
MIPI_CSI_RX_D0N/LVDS_RX_D0N/GPI3_C2_d	86	GPI3
MIPI_CSI_RX_D0P/LVDS_RX_D0P/GPI3_C3_d	87	GPI3
MIPI_AVDD1V8/GPIO7_VCC1V8	88	GPIO7	PWR
VSS	E-PAD	PWR