Adlink nanoX-EL

http://wiki.inmys.ru/start

SATA

SATA0	HSIO 10
SATA1	HSIO 11

PCIe

PCIE0	HSIO 2
PCIE1	HSIO 3
PCIE2	HSIO 4
PCIE3	HSIO 5

LPC

LPC_CLK = 24MHz

LPC Bus is supported by a eSPI-to-LPC bridge IC

USB

USB 0	HSIO 0	from XHCI controller
USB 1	HSIO 1	from XHCI controller