Adlink nanoX-EL

docs

nanoX-EL	Adlink	SOM flyer
nanoX-EL	Adlink	User's guide
PTN3460	NXP	eDP<>LVDS bridge	link

SATA

SATA0	HSIO 10
SATA1	HSIO 11

PCIe

PCIE0	HSIO 2
PCIE1	HSIO 3
PCIE2	HSIO 4
PCIE3	HSIO 5

LPC

LPC_CLK = 24MHz

LPC Bus is supported by a eSPI-to-LPC bridge IC

USB

USB 0	HSIO 0	from XHCI controller
USB 1	HSIO 1	from XHCI controller