Portwell PCOM-BA02GL

docs

PCOM-BA02GL	Portwell	SOM flyer	link
PCOM-BA02GL	Portwell	User's guide	link
PTN3460	NXP	eDP<>LVDS bridge	link
IT5121VG-I-128	ITE	EC
ECE1200	Microchip	eSPI<>LPC	link

USB

USB 0	HSIO 0	from XHCI controller
USB 1	HSIO 1	from XHCI controller

PCIe

PCIE0	HSIO 2
PCIE1	HSIO 3
PCIE2	HSIO 4
PCIE3	HSIO 5

SATA

SATA0	HSIO 10
SATA1	HSIO 11

LPC

LPC Bus is supported by a eSPI-to-LPC bridge IC