Synchronous Internet (Sync-E)

The CLKOUT pin can be assigned to output the recovered clock.

The recovery clock for Sync-E can be either a 125MHz or 25MHz clock.

If the CLKOUT pin is assigned to output the recovered clock from PHY and PHY is working at 1000BASE-T mode, when the PHY is in SLAVE mode, the CLKOUT will output the recoverd clock from the MDI. If the device is in MASTER mode, the CLKOUT will output the clock based on the local free run PLL.

IC	Type	Sync-E	IEEE1588
YT8531S	PHY	+