RS-232

Sitcores	http://en.sitcores.com/index.php?m=content&c=index&a=prolists&catid=41#
ST
TI\Maxim
Analog Devices
Renesas(Intersil)
EXAR
ASIX

ST

Part Number	General Description	Marketing Status	Number of Drivers typ	Number of Receivers typ	Supply Voltage (V) min	Supply Voltage (V) max	Data Rate (kbps) min	Data Rate (kbps) nom	Current Consumption (Icc) (mA) typ	Current Consumption (Icc) (mA) max	ESD: HBM Minimum (V) nom	IEC 61000-4-2 (kV) min	Operating Temperature (°C) min	Operating Temperature (°C) max	Features	Package	Unit Price (US$)
ST202B	5V powered multi-channel RS-232 drivers and receivers	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	-40	85	4 x 0.1uF extenal caps	SO-16, TSSOP-16L	0.4561
ST202C	5V POWERED MULTI-CHANNEL RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	0	70	4 x 0.1uF extenal caps	SO-16	0.3478
ST202EB	15KV ESD PROTECTED 5V RS-232 TRANSCEIVER, [-40oC, 85oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	230	400	5	10	1500, 15000	6	-40	85	-	SO-16, TSSOP-16L	0.5088, 0.5646
ST202EC	15KV ESD PROTECTED 5V RS-232 TRANSCEIVER, [0oC, 70oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	230	400	5	10	1500, 15000	6	0	70	-	SO-16, TSSOP-16L	0.5055, 0.5079
ST232AB	VERY HIGH SPEED, ULTRA LOW POWER CONSUMPTION 5V POWERED RS-232 DRIVERS AND RECEIVERS, [-40oC, 85oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	-40	85	-	SO-16	0.5281
ST232AC	VERY HIGH SPEED, ULTRA LOW POWER CONSUMPTION 5V POWERED RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	0	70	-	SO-16	0.5079
ST232B	5V POWERED MULTI-CHANNEL RS-232 DRIVERS AND RECEIVERS, [-40oC, 85oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	120	220	5	10	1500	-	-40	85	-	SO-16, TSSOP-16L	0.3429, 0.3729
ST232C	5V POWERED MULTI-CHANNEL RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	120	220	5	10	1500	-	0	70	-	SO-16, TSSOP-16L	0.2896, 0.4224
ST232EB	15kV ESD-protected 5 V RS-232 transceiver	Active	2	2	4.5	5.5	230	400	5	10	1500, 15000	6	-40	85	-	SO-16, TSSOP-16L	0.4819, 0.5352
ST232EC	15KV ESD PROTECTED 5V RS-232 TRANSCEIVER, [0oC, 70oC] TEMPERATURE RANGE	Active	2	2	4.5	5.5	230	400	5	10	1500	6	0	70	-	SO-16	0.2936
ST3222B	3 TO 3.6V, LOW POWER, UP TO 400 KBPS RS-232 DRIVERS AND RECEIVERS, [-40oC, 85oC] TEMPERATURE RANGE	Active	2	2	3	3.6	240	400	0.3	1	1999	-	-40	85	-	TSSOP-20	0.7126
ST3222C	3 TO 3.6V, LOW POWER, UP TO 400 KBPS RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE	Active	2	2	3	3.6	240	400	0.3	1	1999	-	0	70	-	TSSOP-20	0.6571
ST3222EB	15kV ESD protected, 3 to 5.5V low power, up to 250Kbps, RS-232 drivers and receivers	Active	2	2	3	5.5	250	-	0.3	1	15000	8	-40	85	-	SSOP 20 7.2×5.3, TSSOP-20	0.8761, 0.9267
ST3222EC	15kV ESD protected, 3 to 5.5V low power, up to 250Kbps, RS-232 drivers and receivers	Active	2	2	3	5.5	250	-	0.3	1	15000	8	0	70	-	SSOP 20 7.2×5.3, TSSOP-20	0.7126, 0.848
ST3232B	3 to 5.5V, low-power, up to 400kbs RS-232 drivers and receivers	Active	2	2	3	5.5	300	400	0.3	2	1999, 2000	-	-40	85	-	SO-16, TSSOP-16L	0.3515, 0.5435
ST3232C	3 to 5.5V, low-power, up to 400kbs RS-232 drivers and receivers	Active	2	2	3	5.5	300	400	0.3	2	1999, 2000	-	0	70	-	SO-16, TSSOP-16L	0.5208, 0.6411
ST3232EB	±15kV ESD protection 3 to 5.5V low power, up to 250kbps, RS-232 drivers and receivers	Active	2	2	3	5.5	250	-	0.3	1	999, 15000	8	-40	85	-	SO-16, TSSOP-16L	0.5853, 0.6282
ST3232EC	±15kV ESD protection 3 to 5.5V low power, up to 250kbps, RS-232 drivers and receivers	Active	2	2	3	5.5	250	-	0.3	1	1500, 15000	8	0	70	-	SO-16, TSSOP-16L	0.5853, 0.6402
ST3237EB	15KV ESP PROTECTED 3 TO 5.5V 250KBPS RS-232 TRANSCEIVER WITH STAND-BY, [-40oC, 85oC] TEMPERATURE RANGE	Active	5	3	3	5.5	1000	-	0.3	1	15000	8	-40	85	-	SSOP 28 10.2×5.3	0.9665
ST3241EB	15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down	Active	3	5	3	5.5	250	-	0.3	1	15000	8	-40	85	Auto-powerdown	SSOP 28 10.2×5.3	1.3702
ST3241EC	15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down	Active	3	5	3	5.5	250	-	0.3	1	15000	8	0	70	Auto-powerdown	SSOP 28 10.2×5.3	1.2293
ST3243C	15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down	Active	3	5	3	5.5	250	400	0.3	1	15000	8	0	70	Auto-powerdown	SSOP 28 10.2×5.3	0.9362
ST3243EB	±15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down	Active	3	5	3	5.5	250	400	0.3	1	15000	8	-40	85	Auto-powerdown	TSSOP-28	0.8758
ST3243EC	±15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down	Active	3	5	3	5.5	250	400	0.3	1	15000	8	0	70	Auto-powerdown	TSSOP-28	1.8114
ST75185C	Multiple RS-232 drivers and receivers	Active	3	5	4.5	5.5	120	-	-	-	1999	-	0	70	-	TSSOP-20	0.2963

ESD

Power

Connectors