RS-232

Sitcores	http://en.sitcores.com/index.php?m=content&c=index&a=prolists&catid=41#
ST
TI\Maxim
Analog Devices
Renesas(Intersil)
EXAR
ASIX

Sitcores

P\N	VCC	Speed, kBps	ESD	TempRange	TX	RX	case	Status
SIT3232E	3.3/5	96	±15	-40~85	2	2	SOP16/SSOP16/TSSOP16/SOPW16	Active
SIT202E	5	120	±15	-40~85	2	2	SOP16	Active
SIT232	5	120	-	-40~85	2	2	SOP16/SSOP16/SSOP16/SOPW16	Active

ST

Part Number	Marketing Status	Number of Drivers typ	Number of Receivers typ	Supply Voltage (V) min	Supply Voltage (V) max	Data Rate (kbps) min	Data Rate (kbps) nom	Current Consumption (Icc) (mA) typ	Current Consumption (Icc) (mA) max	ESD: HBM Minimum (V) nom	IEC 61000-4-2 (kV) min	Operating Temperature (°C) min	Operating Temperature (°C) max	Features	Package	Unit Price (US$)	General Description
ST202B	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	-40	85	4 x 0.1uF extenal caps	SO-16, TSSOP-16L	0.4561	5V powered multi-channel RS-232 drivers and receivers
ST202C	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	0	70	4 x 0.1uF extenal caps	SO-16	0.3478	5V POWERED MULTI-CHANNEL RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE
ST202EB	Active	2	2	4.5	5.5	230	400	5	10	1500, 15000	6	-40	85	-	SO-16, TSSOP-16L	0.5088, 0.5646	15KV ESD PROTECTED 5V RS-232 TRANSCEIVER, [-40oC, 85oC] TEMPERATURE RANGE
ST202EC	Active	2	2	4.5	5.5	230	400	5	10	1500, 15000	6	0	70	-	SO-16, TSSOP-16L	0.5055, 0.5079	15KV ESD PROTECTED 5V RS-232 TRANSCEIVER, [0oC, 70oC] TEMPERATURE RANGE
ST232AB	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	-40	85	-	SO-16	0.5281	VERY HIGH SPEED, ULTRA LOW POWER CONSUMPTION 5V POWERED RS-232 DRIVERS AND RECEIVERS, [-40oC, 85oC] TEMPERATURE RANGE
ST232AC	Active	2	2	4.5	5.5	200	400	1.5	4	1500	-	0	70	-	SO-16	0.5079	VERY HIGH SPEED, ULTRA LOW POWER CONSUMPTION 5V POWERED RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE
ST232B	Active	2	2	4.5	5.5	120	220	5	10	1500	-	-40	85	-	SO-16, TSSOP-16L	0.3429, 0.3729	5V POWERED MULTI-CHANNEL RS-232 DRIVERS AND RECEIVERS, [-40oC, 85oC] TEMPERATURE RANGE
ST232C	Active	2	2	4.5	5.5	120	220	5	10	1500	-	0	70	-	SO-16, TSSOP-16L	0.2896, 0.4224	5V POWERED MULTI-CHANNEL RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE
ST232EB	Active	2	2	4.5	5.5	230	400	5	10	1500, 15000	6	-40	85	-	SO-16, TSSOP-16L	0.4819, 0.5352	15kV ESD-protected 5 V RS-232 transceiver
ST232EC	Active	2	2	4.5	5.5	230	400	5	10	1500	6	0	70	-	SO-16	0.2936	15KV ESD PROTECTED 5V RS-232 TRANSCEIVER, [0oC, 70oC] TEMPERATURE RANGE
ST3222B	Active	2	2	3	3.6	240	400	0.3	1	1999	-	-40	85	-	TSSOP-20	0.7126	3 TO 3.6V, LOW POWER, UP TO 400 KBPS RS-232 DRIVERS AND RECEIVERS, [-40oC, 85oC] TEMPERATURE RANGE
ST3222C	Active	2	2	3	3.6	240	400	0.3	1	1999	-	0	70	-	TSSOP-20	0.6571	3 TO 3.6V, LOW POWER, UP TO 400 KBPS RS-232 DRIVERS AND RECEIVERS, [0oC, 70oC] TEMPERATURE RANGE
ST3222EB	Active	2	2	3	5.5	250	-	0.3	1	15000	8	-40	85	-	SSOP 20 7.2×5.3, TSSOP-20	0.8761, 0.9267	15kV ESD protected, 3 to 5.5V low power, up to 250Kbps, RS-232 drivers and receivers
ST3222EC	Active	2	2	3	5.5	250	-	0.3	1	15000	8	0	70	-	SSOP 20 7.2×5.3, TSSOP-20	0.7126, 0.848	15kV ESD protected, 3 to 5.5V low power, up to 250Kbps, RS-232 drivers and receivers
ST3232B	Active	2	2	3	5.5	300	400	0.3	2	1999, 2000	-	-40	85	-	SO-16, TSSOP-16L	0.3515, 0.5435	3 to 5.5V, low-power, up to 400kbs RS-232 drivers and receivers
ST3232C	Active	2	2	3	5.5	300	400	0.3	2	1999, 2000	-	0	70	-	SO-16, TSSOP-16L	0.5208, 0.6411	3 to 5.5V, low-power, up to 400kbs RS-232 drivers and receivers
ST3232EB	Active	2	2	3	5.5	250	-	0.3	1	999, 15000	8	-40	85	-	SO-16, TSSOP-16L	0.5853, 0.6282	±15kV ESD protection 3 to 5.5V low power, up to 250kbps, RS-232 drivers and receivers
ST3232EC	Active	2	2	3	5.5	250	-	0.3	1	1500, 15000	8	0	70	-	SO-16, TSSOP-16L	0.5853, 0.6402	±15kV ESD protection 3 to 5.5V low power, up to 250kbps, RS-232 drivers and receivers
ST3237EB	Active	5	3	3	5.5	1000	-	0.3	1	15000	8	-40	85	-	SSOP 28 10.2×5.3	0.9665	15KV ESP PROTECTED 3 TO 5.5V 250KBPS RS-232 TRANSCEIVER WITH STAND-BY, [-40oC, 85oC] TEMPERATURE RANGE
ST3241EB	Active	3	5	3	5.5	250	-	0.3	1	15000	8	-40	85	Auto-powerdown	SSOP 28 10.2×5.3	1.3702	15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down
ST3241EC	Active	3	5	3	5.5	250	-	0.3	1	15000	8	0	70	Auto-powerdown	SSOP 28 10.2×5.3	1.2293	15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down
ST3243C	Active	3	5	3	5.5	250	400	0.3	1	15000	8	0	70	Auto-powerdown	SSOP 28 10.2×5.3	0.9362	15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down
ST3243EB	Active	3	5	3	5.5	250	400	0.3	1	15000	8	-40	85	Auto-powerdown	TSSOP-28	0.8758	±15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down
ST3243EC	Active	3	5	3	5.5	250	400	0.3	1	15000	8	0	70	Auto-powerdown	TSSOP-28	1.8114	±15kV ESD protected 3 to 5.5V, 400kbps, RS-232 transceiver with auto power-down
ST75185C	Active	3	5	4.5	5.5	120	-	-	-	1999	-	0	70	-	TSSOP-20	0.2963	Multiple RS-232 drivers and receivers

ESD

Power

Connectors