T1/E1/J1

Renesas

Device	Type	Description	Transformer Selection Group
IDT82V2041E	LIU	T1 / J1 / E1 Single Short Haul	PART 2
IDT82V2042E	LIU	T1 / J1 / E1 Dual Short Haul	PART 2
IDT82V2044	LIU	T1 / E1 Quad Short Haul	PART 1
IDT82V2044E	LIU	T1 / J1 / E1 Quad Short Haul	PART 2
IDT82V2048	LIU	T1 / E1 Octal Short Haul	PART 1
IDT82V2048E	LIU	T1 / J1 / E1 Octal Short Haul	PART 2
IDT82V2048L	AFE	T1 / E1 Octal Analog Front End	PART 1
IDT82V2051E	LIU	E1 Single Short Haul	PART 2
IDT82V2052E	LIU	E1 Dual Short Haul	PART 2
IDT82V2054	LIU	E1 Quad Short Haul	PART 1
IDT82V2058	LIU	E1 Octal Short Haul	PART 1
IDT82V2081	LIU	T1 / J1 / E1 Single Short /Long Haul	PART 2
IDT82V2082	LIU	T1 / J1 / E1 Dual Short /Long Haul	PART 2
IDT82V2084	LIU	T1 / J1 / E1 Quad Short /Long Haul	PART 2
IDT82V2088	LIU	T1 / J1 / E1 Octal Short /Long Haul	PART 2
IDT82P2828	High Density LIU	T1 / J1 / E1 28 (+1) Short Haul	PART 2 (for Differential mode) PART 1 (for Single Ended mode)
IDT82P2821	High Density LIU	T1 / J1 / E1 21 (+1) Short Haul	PART 2 (for Differential mode) PART 1 (for Single Ended mode)
IDT82P2521	High Density LIU	E1 21 (+1) Short Haul	PART 2 (for Differential mode) PART 1 (for Single Ended mode)
IDT82P2816	High Density LIU	T1 / J1 / E1 16 (+1) Short Haul	PART 2 (for Differential mode) PART 1 (for Single Ended mode)
IDT82P2808	High Density LIU	T1 / J1 / E1 8 (+1) Short Haul	PART 2 (for Differential mode) PART 1 (for Single Ended mode)
IDT82P2281	Transceiver	T1 / J1 / E1 Single Short /Long Haul	PART 2
IDT82P2282	Transceiver	T1 / J1 / E1 Dual Short /Long Haul	PART 2
IDT82P2284	Transceiver	T1 / J1 / E1 Quad Short /Long Haul	PART 2
IDT82P2288	Transceiver	T1 / J1 / E1 Octal Short /Long Haul	PART 2
PART1	PART2

LIU Frontend

IDT82P2282

RX PRI:1	TX SEC:2
RX SEC:1	TX PRI:1

География\Стандарт

T1

E1

J1

Дальность линии

Short Haul — короткие линии (до 200 м)

Long Haul — длинные линии (до 1800 м)

Структурные части

AFE - Analog Front End

LIU - Line Interface Unit

Framer

Multiplexor

Форматы линейного кодирования:

AMI

B8ZS

HDB3

Основные отличия стандартов T1, E1 и J1, используемых в цифровой телефонии, заключаются в скорости передачи, количестве каналов и географическом распространении.

Е1 (Европа/Азия)

обеспечивает 30+2 канала со скоростью 2,048 Мбит/с,

T1 (США) и J1 (Япония)

предлагают 24 канала со скоростью 1,544 Мбит/с, различаясь способами формирования потока.

Основные отличия T1, E1, J1:

География и стандарт:

E1 (CEPT): Европа, Азия, включая Россию.

T1 (ANSI): Северная Америка.

J1 (TTC): Япония.

Скорость передачи:

E1: 2,048 Мбит/с.

T1/J1: 1,544 Мбит/с.

Структура каналов (тайм-слоты):

E1: 32 тайм-слота (30 для голоса, 1 для синхронизации, 1 для сигнализации).

T1/J1: 24 тайм-слота по 64 кбит/с.

Кодирование звука:

E1: А-закон (A-law).

T1/J1: μ-закон (mu-law).

Линейное кодирование:

E1: AMI, HDB3.

T1/J1: AMI, B8ZS.