ТЗ на модуль NMS-NV-RK3568 V1

Функциональные требования

Аналог SOM от Nvidia Jetson Nano, Jetson Xavier NX, Jetson TX2 на Процессоре Rockchip RK3568

Jetson Nano	Jetson TX2	Jetson Xavier NX
69.6 x 45 mm	69.6 x 45 mm	69.6 x 45 mm

Структурная схема

Основные компоненты

CPU	RockChip	RK3568	Rockchip RK3568 Datasheet V1.2-20210601.pdf
PMIC	RockChip	rk809-5	Rockchip RK809 Datasheet V1.7 20201014.pdf
ETH PHY	Broadcom	bcm54210peb1imlg	1 gbit RGMII -40…85 48-QFN (7x7x0.85)	MCS54210PE-DS01_8x8.pdf
LPDDR4	Micron	MT53D512M32D2DS-053	16 gbit (2GB) -25…85 200-WFBGA (10×14.5×0.8)	200b_z11m_non_auto_lpddr4_lpddr4x.pdf
EMMC	Kioxia	thgamrg7t13bail	128 gbit (16GB) -25…85 153-WFBGA (11.5×13)	Kioxia_THGAMRG7T13BAIL_BiCS3 16GB_5_1_E_rev3_0_20200210.pdf Digikey
RTC	NXP	PCF8523TK/1,118	PCF8523.pdf
boost DCDC	Onsemi	FAN48623UC50X	3-5.25V→5V	FAIR-S-A0000507963-1.pdf
buck DCDC	Onsemi	NCP1597BMNTWG	5V→3V3	NCP1597B-D.PDF
buck DCDC	Onsemi	FAN53200UC35X	3-5.25→0.9	FAN53200-D.PDF
buck DCDC	Diodes	PAM2305CGFADJ	3-5.25→0.6	PAM2305.pdf
PCIe CLK GEN	Diodes	PI6CG18401	25 MHz XTAL→4x 100MHz	PI6CG18401.pdf
SATA\USB3 SW	Texas Instruments	HD3SS3202	SATA\USB3 switch 1:2	hd3ss3202.pdf
NXP	CBTL02043A	CBTL02043BBQ,115.pdf

Процессор

Rockchip RK3568

RAM

Micron MT53D512M32D2DS-053 - 2 ГБ (16гбит)

Предусмотреть вариант LPDDR4\LPDDR4x - изменение питания 1.1 \ 0.6 В

FLASH

eMMC Kioxia THGAMRG7T13BAIL 16 ГБ 8bit

SDCARD

SDIO 3.0 4 bit

RTC

onboard discrete?

Видеоинтерфейсы

primary	HDMI
secondary	MIPI DSI 4 lines
third	eDP

Ethernet

1 x onboard Gigabit PHY DAPU? (RGMII)

USB 2.0

?x host

USB 3.0

?x device OTG

PCIe 2.1

? lane

PCIe 3.0

? lane

UART

?x (console)

CAN

?x

SPI

?x

I2C

?x

PWM

?x

GPIO

?x

HW Reset

+?

ON\OFF

+?

входное питание

5В	(в SMARC 3-5В)

PMIC

RK809-5

RTC power

ext

Конструктивные требования

Формфактор

Nvidia SOM (Jetson Nano, Jetson Xavier NX, Jetson TX2)

Охлаждение

Предусмотреть 2 отверстия рядом с процессором для лучшего прижима\крепления радиатора

???

Диаметр:

KeepOut:

Примерный внешний вид

Разъёмы

System connector

Краевой разъём: SO-DIMM 260 PIN

Эксплуатационные? требования

temp range	industrial	память, eMMC от -20 - это Industrial?

Разное

Документация

IC-MEM-LPDDR4
link	ext	description	manufacturer	version	date	lang
200b_z11m_non_auto_lpddr4_lpddr4x.pdf	pdf	LPDDR4/LPDDR4X SDRAM MT53D512M16D1, MT53D512M32D2, MT53D1024M32D4 200b: x16/x32 Features	Micron	D 3/20 EN	2017	EN
IC-MEM-eMMC
link	ext	description	manufacturer	version	date	lang
Kioxia_THGAMRG7T13BAIL_BiCS3 16GB_5_1_E_rev3_0_20200210.pdf	pdf	16GB EMMC 11.5×13 153ball	Kioxia	V3.0	2020.02	EN
IC-IF-ETH-PHY
link	ext	description	manufacturer	version	date	lang
BCM54210E-AN102-RDS.pdf	pdf	BCM54210E Design Guide	Broadcom	2015.06	EN
MCS54210PE-DS01_8x8.pdf	pdf	BCM54210E Datasheet	Broadcom	2020.03	EN
IC-IF-SWITCH
link	ext	description	manufacturer	version	date	lang
hd3ss3202.pdf	pdf	HD3SS3202 Two-Channel Differential 2:1/1:2 USB3.1 Mux/Demux SLASEO1A –MAY 2018–REVISED SEPTEMBER 2018 HD3SS3202IRSVR HD3SS3202IRSVT HD3SS3202RSVR HD3SS3202RSVT	Texas Instruments	rev. A	2018.09	EN
IF-FREQ-CLKGEN
link	ext	description	manufacturer	version	date	lang
PI6CG18401.pdf	pdf	PI6CG18401 Diodes Very Low Power 4-Output PCIe Clock Generator With On-chip Termination	Diodes	rev 3-2	2022.01	EN
IC-FREQ-RTC
link	ext	description	manufacturer	version	date	lang
PCF8523.pdf	pdf	PCF8523 NXP Real-Time Clock (RTC) and calendar Rev. 7 — 28 April 2015	NXP	rev. 7	2015.04	EN
IC-POW-DCDC
link	ext	description	manufacturer	version	date	lang
FAN53200-D.PDF	PDF	FAN53200 Onsemi TinyBuck Regulator, Digitally Programmable, 5 A, 2.4 MHz	Onsemi	rev. 3	2020.05	EN
FAIR-S-A0000507963-1.pdf	pdf	FAN48623 Onsemi (Fairchild) 2500 mA Boost DCDC with Bypass Mode	Onsemi (Fairchild)	rev. 1.7	2015.03	EN
NCP1597B-D.PDF	PDF	NCP1597B Onsemi Buck Regulator - Synchronous 1 MHz, 2 A	Onsemi	rev. 2	2019.08	EN
PAM2305.pdf	pdf	PAM2305 Diodes 1A STEP-DOWN DC-DC CONVERTER	Diodes	rev. 2-6	2013.01	EN

Разная инфа