Freq

http://mxtal.ru/ru/	ООО «Мэджик Кристалл»	Омск
https://bmgplus.ru/	НПФ «БМГ ПЛЮС»	Москва
https://morion.com.ru/	Морион	СПб
https://www.electronshik.ru/item/YXC	YXC
https://www.sztkd.com/index.html	TKD	XTAL, RTC, TXCO, OXCO
https://www.chinafronter.com/	chinafronter	XTAL, TXCO, OXCO, etc
https://www.microcrystal.com/	Micro Crystal	XTAL, RTC, TXCO, OXCO
https://www.xtalong.com/	xtalong	XTAL, XCO, TXCO
http://www.conwin.com/	Connor Winfield	OCXO, …
http://www.abracon.com/	Abracon	OCXO, …
Vectron	OCXO, …
NDK	OCXO, …

156.25 = 625/4

XTAL

32 KHz	-40…+85	3.2×1.5	YXC	https://www.electronshik.ru/item/YXC/X321532768KGD2SI	~ 10р	ABS07-32.768KHZ-T
25 MHz	-40…+85	3.2×2.5	YXC	https://www.electronshik.ru/item/YXC/X322525MOB4SI	~5р

XCO

OCXO

http://www.conwin.com/datasheets/cx/cx309.pdf

Abracon	AOC1409	14.9×9.7×7
Abracon	AOC2012	20×12.7×11
Abracon	AOC2522	25.4x22x12
Abracon	AOCJYR	9.7×7.5×4.3
Abracon	AOCJY	25.5×22.1×12.5
Abracon	AOCJY2	21x21x11
Abracon	AOCJY3	25.4×25.4×13
TKD	TOC-2525	25x25x14.8	10.000MHz-100.000MHz
TKD	TOC-1409	14x9x6.5	10.000-40.000MHz
TKD	TOC-0907	9x7x4.1	10.000-40.000MHz
Connor-Winfield	OH100
Connor-Winfield	OH200
Connor-Winfield	OH300
Connor-Winfield	OH320
Connor-Winfield	DOC

NDK ENE3311A

CTS OSC5A2B02

EBAY: PCBA GPSDO Board GPS Disciplined Oscillator 10M Frequency Reference GNSS 1PPS

XCO diff

https://www.sztkd.com/uploadfile/2022/0714/20220714112059269.pdf	TKD	LVDS\HCSL\LVPECL	1-125 MHz	0.1ps jitter

RTC

https://www.sztkd.com/uploadfile/2022/0923/20220923093614837.pdf	TKD	1.65-5.5V	int xtal
RV-3032-C7	2.5ppm	-40+85C	1.98$ (при заказе 3000 шт.)
DaPu	INS5699C	3.4ppm	-40+85C	1.49$ (при заказе 3000 шт.)	(RTC TCXO SMD3225 32.768kHz 1.6-5.5V I2C)
DaPu	INS5699S	5ppm	-40+85C	1.298$ (при заказе 3000 шт.)	(RTC TCXO SMD3225 32.768kHz 2.5-5.5V I2C)

CLK BUF\MUX

link	ext	description	manufacturer	version	date	lang
PI6C485352.pdf	pdf	PI6C485352 2.5/3.3V, 500MHz 12 2-to-1 diff LVPECL clock MUX	PERICOM	Rev. A	2013.01	EN

CLK GEN

Diodes
link	ext	description	manufacturer	version	date	lang
Diodes_Inc.-PI6CG184Q2ZHQEX-datasheet.pdf	pdf	PI6CG184Q 4-Output PCIe Gen 4 Clock Generator for Automotive Applications Diodes	Diodes	rev 2-2	2020.02	EN
Diodes_Inc.-PI6CG18401ZHIEX-datasheet.pdf	pdf	PI6CG18401 Very Low Power 4-Output PCIe Clock Generator With On-chip Termination	Diodes	rev 2-2	2020.06	EN
PI6CG18401.pdf	pdf	PI6CG18401 Very Low Power 4-Output PCIe Clock Generator With On-chip Termination Diodes	Diodes	rev 3-2	2022.01	EN