ETH PHY

Производители

Voltage mode or Current mode Ethernet PHY

http://localhost/hash/6bf998c0c755a8c4e32568699476fbde/slyp788.pdf

10/100Mbit, 2 Channels, 3.3V center tab	10/100Mbit, 2 Channels
3.3V*40mA= 132mA * 2 channels = 264mA	3.3V*6mA= 19.8mA * 2 channels = 39.6mA
1000Mbit, 4 Channels, 3.3V center tab	1000Mbit, 4 Channels
3.3V*40mA= 132mA * 4 channels = 528mA	3.3V*6mA= 19.8mA * 4 channels = 79.2mA

Микросхемы

Chip	Manufacturer	Interface	Speed	Operating t	Octopart	DKO el	Datasheet	I/O levels	Comment
B50210E	Broadcom	RGMII	10/100/1000	-40; +85	Octopart	DKO	b50210e-ds06.pdf	1.8V HSTL, 2.5V 3.3V
BCM54210E	Broadcom	RGMII, SGMII	10/100/1000	-40; +85	Octopart	DKO	bcm54210e-ds07.pdf bcm54210e-an102-rds.pdf	1.8V HSTL, 2.5V 3.3V
BCM54811A2IMLG	Broadcom	GMII, RGMII, SGMII	10/100/1000	Octopart	DKO	bcm54811.pdf
BCM5461S	Broadcom	GMII, RGMII, SGMII	10/100/1000	Octopart	DKO
BCM54616S	Broadcom	RGMII, SGMII	10/100/1000	Octopart	DKO
BCM54210S	Broadcom	RGMII, SGMII	10/100/1000	-40; +85	Octopart	DKO	2.5V 3.3V
KSZ9021RNI	Microchip	RGMII	10/100	-40;+85	Octopart	DKO
KSZ9031RNXIA	Microchip	MII, RGMII, GMII	10/100/1000	-40;+85	Octopart	DKO	ksz9031rnxia.pdf	1.8V 2.5V 3.3V
KSZ9131RNXV	Microchip	GMII,MII,RGMII	10/100/1000	-40;+105	Octopart	DKO	ksz9131rnxi.pdf	1.8V 2.5V 3.3V
LAN8820i	Microchip	GMII,MII,RGMII	10/100/1000	-40;+85	Octopart	DKO	lan8820.pdf	2.5V
LAN8742AI	Microchip	RGMII	10/100	-40;+85	Octopart	DKO	lan8742ai.pdf	1.8V 2.5V 3.3V
LAN8720AI	Microchip	RMII	10/100	-40;+85	Octopart	DKO	lan8720ai.pdf	1.8V 2.5V 3.3V
LAN8700	Microchip	MII RMII	10/100	0;+70	Octopart	DKO	lan8700c_i_.pdf	1.8V 2.5V 3.3V
LAN8700I	Microchip	MII RMII	10/100	-40;+85	Octopart	DKO	lan8700c_i_.pdf	1.8V 2.5V 3.3V
ADIN1200	Analog Devices	MII, RMII, RGMII	10/100	-40;+105	Octopart	DKO	adin1200.pdf	1.8V 2.5V 3.3V
ADIN1300	Analog Devices	MII, RMII, RGMII	10/100/1000	-40;+105	Octopart	DKO	adin1300.pdf	1.8V 2.5V 3.3V
AR8031-AL1B	Atheros	RGMII, SGMII	10/100/1000	-40;+85	Octopart	DKO	ar8031.pdf	1.5V 1.8V 2.5V 3.3V
AR8033-AL1B	Atheros	RGMII	10/100/1000	-40;+85	Octopart	DKO
AR8035-AL1B	Atheros	RGMII	10/100/1000	-40;+85	Octopart	DKO
VSC8501XML-03	Microsemi	RGMII	10/100/1000	-40;+125	Octopart	DKO	vsc8501xml-03.pdf
VSC8531XMW-02	Microsemi	RGMII	10/100/1000	-40;+125	Octopart	DKO	vsc8531-02.pdf	1.5V 1.8V 2.5V 3.3V
VSC8541XMV-05	Microsemi	RGMII	10/100/1000	-40;+125	Octopart	DKO	vsc8541xmv-05.pdf	1.5V 1.8V 2.5V 3.3V
DP83620	TI	RMII, MII	10/100	-40;+85	Octopart	DKO	dp83620.pdf	2.5V 3.3V
DP83822	TI	RGMII, RMII, MII	10/100	-40;+125	Octopart	DKO
DP83867IR	TI	RGMII, GMII, MII	10/100/1000	-40;+85	Octopart	DKO
88E1510-A0-NNB2I	Marvell	RGMII, SGMII	10/100/1000	-40;+85	Octopart	DKO	88e151x	2.5V 3.3V
88E1518	Marvell	RGMII, SGMII	10/100/1000	0;+70	Octopart	DKO	88e151x	1.8V
88E1512-A0-NNP2I	Marvell	RGMII, SGMII	10/100/1000	-40;+85	Octopart	DKO	88e151x	1.8V 2.5V 3.3V
PEF7072	Rochester Electronics / Latniq / Intel	RGMII, SGMII	10/100/1000	Octopart	DKO	У Вани остались не самые приятные впечатления от работы с этим модулем
TJA1100	NXP	1000	Octopart	DKO
TJA1101	NXP	1000	Octopart	DKO
RTL8211FI / RTL8211FDI	Realtek	RGMII	10/100/1000	-40;+85	Octopart	DKO	rtl8211fi.pdf
DM9119INP	Davicom	GMII/RGMII	10/100/1000	-40;+85	Octopart	DKO	dm9119inp.pdf	2.5V 3.3V
DM9119INX	Davicom	GMII/RGMII	10/100/1000	-40;+85	Octopart	DKO	pdf	2.5V 3.3V
DAP8211R	Dapu	RGMII	10/100/1000	0;+70	ETH PHY	ETH PHY	https://www.dptel.hk.cn/Products/ProductLevel3/1938
DAP8211RI	Dapu	RGMII	10/100/1000	-40;+85?

WiFi

AP6212	Octopart	DKO	ap6212.pdf

I219V I219LM

Chip	Manufacturer	Interface	Speed	Operating t	Octopart	DKO el	Datasheet	I/O levels	Comment
WGI219V	Intel	PCIe like	10/100/1000	0…+85	Octopart	DKO	http://wiki.inmys.ru/start	3.3V
WGI219LM	Intel	PCIe like	10/100/1000	0…+85	Octopart	DKO	http://wiki.inmys.ru/start	3.3V