USB switch\mux\crossbar

link	ext	description	manufacturer	version	date	lang
CBTL04GP043EXJ.pdf	pdf	CBTL04GP043 Dual 2 x 2 differential channel crossbar switch XFBGA28 2x4mm Rev. 1 — 24 October 2014 Product data sheet	NXP	rev. 1	2014.10	EN
CBTL02043BBQ,115.pdf	pdf	CBTL02043A; CBTL02043B 3.3 V, 2 differential channel, 2 : 1 multiplexer/demultiplexer switch QFN20 2.5×4.5mm Rev. 4.1 — 30 March 2015 Product data sheet	NXP	rev. 4.1	2015.03	EN
CBTU02043HEJ.pdf	pdf	CBTU02043 High-speed differential 1-to-2 switch HUQFN16 1.6×2.4mm Rev. 3 — 19 July 2018 Product data sheet	NXP	rev. 3	2018.07	EN
hd3ss3202.pdf	pdf	HD3SS3202 Two-Channel Differential 2:1/1:2 USB3.1 Mux/Demux UQFN16-1.8×2.6mm SLASEO1A –MAY 2018–REVISED SEPTEMBER 2018 HD3SS3202IRSVR HD3SS3202IRSVT HD3SS3202RSVR HD3SS3202RSVT	Texas Instruments	rev. A	2018.09	EN
NL3HS3124A-D.PDF	PDF	NL3HS3124A 3.3 V, 2 Channel, 2:1 Differential Mux/Demux QFN20 2.5×4.5mm	Onsemi	rev. 1	2016.12	EN
ts3usb221.pdf	pdf	TS3USB221 High-speed USB 2.0 (480-Mbps) 1:2 multiplexer – demultiplexer switch with single enable SCDS220J –NOVEMBER 2006–REVISED JANUARY 2019	Texas Instruments	rev. J	2019.01	EN