DSI

TE - tearing effect

The tearing effect allows a perfect synchronization between the display and the DSI Host for refresh operations on displays having their own Graphics RAM. The tearing effect can be signaled in two ways: - Over the link without an additional pin, - Or using an additional pin.

SMARC