Упаковка ЭК

Onsemi	https://www.onsemi.com/pub/collateral/brd8011-d.pdf
Analog	https://www.analog.com/media/en/package-pcb-resources/tape-and-reel-packaging.pdf
MiniCircuits	https://www.minicircuits.com/pdfs/tape_reel.pdf
TI	https://www.ti.com/lit/ug/snoa403i/snoa403i.pdf
Vishay	https://www.vishay.com/docs/88869/packaging.pdf
Diodes	https://www.diodes.com/assets/Tape%20Reel%20Files/tapereel_2.pdf
Renesas	https://www.renesas.com/us/en/document/oth/tb347-tape-and-reel-specification-integrated-circuits
KOAspeer	https://www.koaspeer.com/pdfs/Appendix_A.pdf
ST	https://www.st.com/resource/en/technical_note/tn1173-packing-information-for-ipad-protection-rectifiers-thyristors-and-ac-switches-stmicroelectronics.pdf

REEL - Катушки

SMD компоненты

reel size

7 inch (178mm, 180mm, 185mm)

2.4 inch hub

12 inch (255mm, 260mm)

13 inch (330mm)

4 inch hub

6 inch hub

14 inch (380mm)

tape width

REEL8 - 8mm tape

2 - pitch

4 - pitch

8 - pitch

REEL12 - 12mm tape

REEL16 - 16mm tape

REEL24 - 24mm tape

REEL32 - 32mm tape

REEL44 - 44mm tape

REEL56 - 56mm tape

REEL72 - 72mm tape

REEL88 - 88mm tape

tape pitch

1

2

4

8

12

16

20

24

32

36

40

Onsemi

годится ли вместо NCP1589AMNTWG вариант NCP1589AMNTXG ?

NOTE: Pin 1 orientation for TWG Suffix is Quadrant 1, upper left; Pin 1 orientation for TXG Suffix is Quadrant 2, upper right

TAPE - Лента?

TRAY - Поддон?

TUBE - Туба?

Внешняя ширина:

8 mm

10 mm

16 mm