Материалы ПП

HVLP copper roughness

TUC-933 (a.k.a T3), HVLP copper foil

TUC-883 (a.k.a T2), HVLP copper foil

Doosan DS-7409DV(N), HVLP copper foil

Doosan DS-7409DV, HVLP copper foil

Standard Loss	Mid-Loss	Low-Loss	Very Low-Loss	Ultra Low-Loss	High Frequency	Others
S1170	S1150G	S7439	Synamic 6	Megtron-7/-7NE	S7135	Embedded Capacitance
S1141/S1140F	S7045G	Megtron-4/M4S	Megtron-6/-6G	TU933/933+	S7136H	3M C-PLY
S1140F	S7038	Megtron-M	Megtron-6NE	EM891K	RO4350B	Dupont HK04J
S1000H	S7040G	TU863/863+	TU-883	DS7409DV(N)	RO4003C	OKA-Mitsui
S1000-2/-2M	HE679G	TU872LK/SLK	I-TERA	IT968-SE	RO3003	Faradflex BC12M, BC24M
S1190	Megtron 2	TU-827SLK SP	Chronon LDK	LW910G	RO3006	Embedded Resistance
EM-285/-825	R1566W	FR408/-408HR	EM-888K	Tachyon-100G	RO4360G2	Ohmega-Ply
EM-827	TU862S	I-Speed	EM891	Synamic 6N	TC350	Asahi Tu-50/1000-08
TU662	TU862HF	N4000-13 Series	LW900G	MW4000	RF35	Hybrid
TU768	IT170GRA1	EM-888/-S	FL700	FL700LD	RF35A2	M6+S1000-2
IT158	IT-150GS	EM-828/828G	DS7409DV	RF60TC	M6+370HR/EM-827
IT180I/IT180A	EM370(D)	IT-150DA	MW2000/3000	RF60A	RO4350B+EM827/370HR
370HR	EM285	IT200LK	IT-968	TLY-5A	RO4360G2+EM827/370HR
E-679(W)	EM-355(D)	NPG-170D	Diclad880	TU-872SLK+TU-768
E-679F(J)	NPG-170N	HE-679G(S)	Cuclad6700	TU-872SLK+TU-862HF
R-1755V	NPG-150N	S7439+S1000-2/S1190
/R1755C	IS415	S7135+S1000-2
TU872SLK+TU768/TU862HF
S7136H+EM827/S1000-2M/S7045G
High Speed	Material	Comment	ds
TUC	TU-872 SLK(TU-87P SLK)	Low Dk/Df and High Thermal Reliability Material Core: TU-872 SLK; Prepreg: TU-87P SLK	link
Panasonic	R-1755V
Panasonic	R-1650V
Panasonic	MC-100MS/EX
Panasonic	MC-Rheopreg
Doosan	7409SN
Doosan	7408
Isola	Tachyon 100G
Isola	Terra Green
Isola	I-tera MT40
Isola	I-Speed
Isola	FR408HR
Isola	IS415
Arlon	35N
Arlon	85N
Standart	Material	Comment	ds
Doosan	7402
Isola	370HR
Isola	IS620i
Isola	FR408HR
Isola	FR408
Isola	IS410
Isola	FR406
Isola	P96
Isola	185HR
Shengyi Technology Co, Ltd.	S1000-2M	LEAD-FREE COMPATIBLE FR-4	link
TUC	TU-768(TU-768P)	High-Tg and High Thermal Reliability Laminate and Prepreg Core: TU-768; Prepreg: TU-768P	link
Гибкие и гибко-жёсткие	Material	Comment	ds
DuPont
Expanex
SDFlex
3M
Hanwha
Теплонагруженные и на основе металла	Material	Comment	ds
CCAF
Bergquist
Laird
Ventec
ShenYi
ITEQ
Rogers
ISOLA
RF	Material	Comment	ds
Rogers	RO4350B
Rogers	RO4003C
Wang-Ling	F4BMX	(доступная замена Rogers и ФАФ-4Д)
Taconic	TLX-9
Taconic	RF-30A
Taconic	RF-35
Taconic	RF-60A